

QMK program

simple: PAUSE ----DEL


open <http://qmkeyboard.cn/>



2 click pause




3



ok，layout is modify download layout

4





5






install software ，


6 PCB get into BootLoader mode


fn+backspace or There is a rest button below the PCB

 or 


7. install drive










8 update hex









complete